{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":17,"n_cols":3,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
["Yes","unswitched power to relay board, power relay","Key off.  Pin 12 on connector - 12v"]
["Yes","Switched power to relay board","Key on.  Pin 8 on  connector - 12v"]
["Yes","Trace relay board connection, pi 14 to power relay","Key off. Power pin10 – 12v"]
["Yes","Test relay board ground","Key off.  Continuity from pin10 to ground"]
["Yes","Connection from pin 10 to power relay pin 86","Key off.  Connector in, pin 86 to ground"]
["Yes","Test power relay","Key off.  Connector in. Power relay pin 87a – 12v"]
["Yes","Unswitched power to fuel pump relay","Key off.  Connector out,  Pin 14 – 12v"]
["Yes","Connection from pin 14 to fuse","Key off.  Power to fuse, both sides"]
["Yes","Connection from fuse to fuel pump pin 30","Key off  Check power at pump relay pin 30 – 12v"]
["Yes","Power to fuel pump relay pin  85","Key on.  Voltage at fuel pump relay pin 85 - 12v"]
["Yes","Connectivity, fuel pump relay pin 86 to 4 pin III","Key off.  Continuity,  pin 86 to ground"]
["Yes","Connectivity, fuel pump relay pin 87a to pin 13","Key off .  Continuity, pin 87a to pin 13"]
["Yes","Fuel pump relay","Key off.  Connector in, voltage at pin 87a = 12v"]
["Yes","Fuel pump ground, wire at pump","Key off.  Continuity, brown wire to ground"]
["No","Fuel pump harness","Key on.  Voltage at fuel pump – Zero"]
["Yes","Fuel pump test","Connect fuel pump to battery – pump runs."]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}